Jump to main content

##

# 1.2 ADCHS Interrupt

This example application shows how to sample an analog input using the ADCHS peripheral and displays the converted samples on a serial terminal.

## Description

In this application, an analog input is converted by a hardware trigger generated by the TMR peripheral. Result is read in the conversion complete interrupt handler. Converted digital value is displayed on the serial terminal.

## Downloading and Building the Application

To clone or download this application from Github, go to the main page of this repository and then click Clone button to clone this repository or download as zip file. This content can also be downloaded using content manager by following these instructions.

Path of the application within the repository is apps/adchs/adchs_interrupt/firmware.

To build the application, refer to the following table and open the project using its IDE.

Project Name | Description
--- | ---
pic32mz_ef_sk.X | MPLABX project for PIC32MZ Embedded Connectivity with FPU (EF) Starter Kit

## Setting Up the Hardware

The following table shows the target hardware for the application projects.

Project Name | Description
--- | ---
pic32mz_ef_sk.X | PIC32MZ Embedded Connectivity with FPU (EF) Starter Kit

### Setting Up PIC32MZ Embedded Connectivity with FPU (EF) Starter Kit

- Connect the AN3 pin RB3 (Pin 15 of the J12) to the VCC (Pin 1 of the J12)
- Connect the COM port J11(USB to UART) to the computer using a mini USB cable
- Connect the Debug USB port on the board to the computer using a mini USB cable

## Running the Application

1. Open the Terminal application (Ex.: Tera term) on the computer
2. Connect to the “USB to UART” COM port and configure the serial settings as follows:
   - Baud : 115200
   - Data : 8 Bits
   - Parity : None
   - Stop : 1 Bit
   - Flow Control : None
3. Build and Program the application project using its IDE
4. Console displays the ADC count and the ADC input voltage