Jump to main content

##

# 3.3.22.10 DT_PADDING Macro

## C

    #define DT_PADDING           (int16_t)12

## Summary

Defines the constant value used as padding for the dead time count in PWM calculations

## Description

This macro defines a constant value used as padding for the dead time count in PWM calculations. It is primarily used to ensure there is an adequate buffer to account for any discrepancies or additional requirements in the PWM dead time configuration

## Remarks

Note:

- Ensure that the value of `DT_PADDING` is appropriate for the specific application and hardware being used.
- The padding value should be chosen based on the timing requirements and constraints of the PWM signals in the application.