Jump to main content

##

# 3.3.20.3 LDMINUSLQ_VS_IS Macro

## C

    #define  LDMINUSLQ_VS_IS  { \
        { 0.0f,  0.00032f }, \
        { 1.0f,  0.00032f }, \
        { 2.0f,  0.00032f }, \
        { 3.0f,  0.00032f }, \
    }

## Summary

Defines the PMSM motor inductance characteristic curves.

## Description

This macro defines a two-dimensional array of data points representing the relationship between the stator current and the difference between the direct-axis inductance (Ld​) and quadrature-axis inductance (Lq​).This data is used in Maximum Torque Per Ampere (MTPA) calculations.

## Remarks

None