Jump to main content

##

# 1.2.5.59 SPW_PKTTX_INT_MASK

    typedef enum
    {
        SPW_PKTTX_INT_MASK_DEACT = SPW_PKTTX1_PI_R_DEACT_Msk,
        SPW_PKTTX_INT_MASK_ACT = SPW_PKTTX1_PI_R_ACT_Msk,
        SPW_PKTTX_INT_MASK_EOP = SPW_PKTTX1_PI_R_EOP_Msk,
        SPW_PKTTX_INT_MASK_EEP = SPW_PKTTX1_PI_R_EEP_Msk,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_PKTTX_INT_MASK_INVALID = 0xFFFFFFFF
    } SPW_PKTTX_INT_MASK;

Summary

Identifies the SPW PKTTX current interrupt status

Description

This data type identifies the SPW PKTTX interrupt status