Jump to main content

##

# 1.2.5.60 SPW_PKTTX_NXTSEND_START

    typedef enum
    {
        SPW_PKTTX_NXTSEND_START_EVENT = SPW_PKTTX1_NXTSENDCFG_START_STARTEVENT_Val,
        SPW_PKTTX_NXTSEND_START_NOW = SPW_PKTTX1_NXTSENDCFG_START_STARTNOW_Val,
        SPW_PKTTX_NXTSEND_START_TCH1 = SPW_PKTTX1_NXTSENDCFG_START_STARTTCH1_Val,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_PKTTX_NXTSEND_START_INVALID = 0xFFFFFFFF
    } SPW_PKTTX_NXTSEND_START;

Summary

Identifies the SPW PKTTX next send list start mode

Description

This data type identifies the SPW PKTTX next send list start mode