Jump to main content

##

# 1.2.5.39 SPW_RMAP_STATUS

    typedef enum
    {
        SPW_RMAP_STATUS_ERRCODE_MASK = SPW_RMAP1_STS_RC_ERRCODE_Msk,
        SPW_RMAP_STATUS_VALID = SPW_RMAP1_STS_RC_VALID_Msk,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_RMAP_STATUS_INVALID = 0xFFFFFFFF
    } SPW_RMAP_STATUS;

Summary

Identifies the SPW RMAP current status

Description

This data type identifies the SPW RMAP status