Jump to main content

##

# 1.2.5.76 SPW_TCH_ConfigureWatchdog

    void SPW_TCH_ConfigureWatchdog(uint16_t earlyNumTick, uint16_t lateNumTick)

Summary

Set SPW TCH watchdog configuration for early and late watchdog interrupts

Preconditions

None

Parameters

- earlyNumTick - Trigger watchdog if new Time Code before this number of tick (TimeTick clock)
- lateNumTick - Trigger watchdog if No new Time Code is received before this number of tick (TimeTick clock)

Returns

None