Jump to main content

##

# 1.1.5.68 SPW_TCH_INT_MASK

    typedef enum
    {
        SPW_TCH_INT_MASK_TCEVENT = SPW_TCH_PI_RM_TCEVENT_Msk,
        SPW_TCH_INT_MASK_TIMECODE = SPW_TCH_PI_RM_TIMECODE_Msk,
        SPW_TCH_INT_MASK_ANYTIMECODE = SPW_TCH_PI_RM_ANYTIMECODE_Msk,
        SPW_TCH_INT_MASK_LATEWD = SPW_TCH_PI_RM_LATEWD_Msk,
        SPW_TCH_INT_MASK_EARLYWD = SPW_TCH_PI_RM_EARLYWD_Msk,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_TCH_INT_MASK_INVALID = 0xFFFFFFFF
    } SPW_TCH_INT_MASK;

Summary

Identifies the SPW TCH Interrupt status mask.

Description

This data type identifies the SPW TCH Interrupt status mask.