Jump to main content

##

# 1.1.5.29 SPW_ROUTER_PHYS_ADDR

    typedef enum
    {
        SPW_ROUTER_PHYS_ADDR_DISABLE = 0,
        SPW_ROUTER_PHYS_ADDR_LINK_1 = SPW_ROUTER_LINK1_PORT,
        SPW_ROUTER_PHYS_ADDR_LINK_2 = SPW_ROUTER_LINK2_PORT,
        SPW_ROUTER_PHYS_ADDR_PKTRX = SPW_ROUTER_PKTRX_PORT,
        SPW_ROUTER_PHYS_ADDR_RMAP = SPW_ROUTER_RMAP_PORT,
        /* Force the compiler to reserve 32-bit memory for enum */
        SPW_ROUTER_PHYS_ADDR_INVALID = 0xFFFFFFFF
    } SPW_ROUTER_PHYS_ADDR;

Summary

Identifies the SPW ROUTER table physical address

Description

This data type identifies the SPW ROUTER table physical address