Jump to main content

##

# 2.120.1.51 TCx_Capture16bitChannel1Get Function

## C

    /* x = TC instance number */
    uint16_t TCx_Capture16bitChannel1Get( void );

## Summary

Reads capture value from channel 1.

## Description

This function reads the captured value stored in CC[1]. Value can be read from interrupt routine or by polling.

## Precondition

TCx_CaptureInitialize() function must have been called first.

## Parameters

None.

## Returns

Captured value from channel 1

## Example

    uint16_t captureValue = 0;
    TC0_CaptureInitialize();
    TC0_CaptureStart();
    captureValue = TC0_Capture16bitChannel1Get();

## Remarks

None.