Jump to main content

##

# 2.100.10 RTC_INT_MASK Enum

## C

    typedef enum
    {
        RTC_INT_ALARM
    } RTC_INT_MASK;

## Summary

Mask for enabling and disabling the RTCC interrupt.

## Description

This enumeration defines the mask for enabling and disabling the RTCC interrupt via IEC5 register. Used by RTCC_InterruptEnable and RTCC_InterruptDisable functions.

## Remarks

This enum is kept to satisfy the drivers which expects an input parameter for RTCC interrupt enable/disable functions. Such enum is used on devices on which the peripheral supports multiple interrupts.