Jump to main content

##

# 2.64.23 MCANx_SleepModeEnter Function

## C

    void MCANx_SleepModeEnter(void) // x - Instance of the MCAN peripheral

## Summary

Puts the MCAN Peripheral in sleep mode (clock stop request).

## Precondition

MCANx_Initialize and MCANx_MessageRAMConfigSet must have been called for the associated MCAN instance.

## Parameters

None.

## Returns

None.

## Example

    MCAN0_SleepModeEnter();

## Remarks

None.