Jump to main content

##

# 2.31.21 DMA_Deinitialize Function

## C

    void DMA_Deinitialize( void )

## Summary

De-initializes the DMA controller of the device to POR Values.

## Description

This function de-initializes the DMA controller control and status registers to it's POR state.

## Precondition

The DMA module clock requirements should have been configured in the MHC Clock Manager utility.

## Parameters

None.

## Returns

None.

## Example

    DMA_Deinitialize();

## Remarks

None