Jump to main content

##

# 2.44.7 EVSYS_InterruptDisable Function

## C

    void EVSYS_InterruptDisable( EVSYS_CHANNEL channel, EVSYS_INT_MASK interruptMask )

## Summary

Disables EVSYS interrupt

## Description

This function disables the specified EVSYS interrupt.

## Precondition

EVSYS module should be initialized with the required configuration parameters from the MCC GUI in the EVSYS_Initialize() function

## Parameters

Param | Description
--- | ---
channel | Channel for which the interrupt needs to be disabled
interrupt | Interrupt to be Disabled

## Returns

None

## Example

    // Disable Event System channel 2 Event Detection interrupt
    EVSYS_InterruptDisable(EVSYS_CHANNEL_2, EVSYS_INT_EVENT_DETECT);

## Remarks

Interrupts configuration will be generated in EVSYS_Initialize() function as per user settings in MCC. The EVSYS_InterruptEnable and EVSYS_InterruptDisable API should be used to enable and disable interrupt at run time.