Jump to main content

##

# 2.3.68 ADCx_ChannelResultInterruptEnable Function

## C

    // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.
    inline static void ADCx_ChannelResultInterruptEnable(ADCx_CHANNEL channel);

## Summary

Enables individual channel interrupt.

## Description

This function enables individual channel interrupt.

## Precondition

None.

## Parameters

Param | Description
--- | ---
channel | Selected channel

## Returns

None.

## Example

    ADC1_ChannelResultInterruptEnable(ADC1_CHANNEL channel);

## Remarks

None.