Jump to main content

##

# 2.121.59 TCCx_PWMStop Function

## C

    /* x = TCC instance number */
    void TCCx_PWMStop( void );

## Summary

Stops PWM generation of given TCC instance

## Description

This function stops the counter of associated instance.

## Precondition

TCCx_PWMInitialize() function must have been called first for the given instance.

## Parameters

None

## Returns

None.

## Example

    TCC0_PWMInitialize();
    TCC0_PWMStart();
    // Run application
    TCC0_PWMStop();

## Remarks

Due to synchronization, there is a delay from writing to register until peripheral is stopped. This function waits till sync operation is complete.