Jump to main content

##

# 2.99.66 RTC_PERIODIC_INT_MASK Enum

## C

    typedef enum
    {
        /* Periodic Interrupt at 128 Hz (RTC Clock Frequency/8) - Prescaler Bit 0 */
        RTC_PER0_MASK,

        /* Periodic Interrupt at 64 Hz (RTC Clock Frequency/16) - Prescaler Bit 1 */
        RTC_PER1_MASK,

        /* Periodic Interrupt at 32 Hz (RTC Clock Frequency/32) - Prescaler Bit 2 */
        RTC_PER2_MASK,

        /* Periodic Interrupt at 16 Hz (RTC Clock Frequency/64) - Prescaler Bit 3 */
        RTC_PER3_MASK,

        /* Periodic Interrupt at 8 Hz (RTC Clock Frequency/128) - Prescaler Bit 4 */
        RTC_PER4_MASK,

        /* Periodic Interrupt at 4 Hz (RTC Clock Frequency/256) - Prescaler Bit 5 */
        RTC_PER5_MASK,

        /* Periodic Interrupt at 2 Hz (RTC Clock Frequency/512) - Prescaler Bit 6 */
        RTC_PER6_MASK,

        /* Periodic Interrupt at 1 Hz (RTC Clock Frequency/1024) - Prescaler Bit 7 */
        RTC_PER7_MASK
    } RTC_PERIODIC_INT_MASK;

## Summary

Possible Periodic Interrupt Mask.

## Description

This enumeration defines the possible periodic interrupt mask.

## Remarks

None.