Jump to main content

##

# 2.129.13 TWIHSx_NACKDataPhase Function

## C

    /* x = TWIHS instance number */

    /* TWIHS slave mode */
    void TWIHSx_NACKDataPhase(bool isNACKEnable)

## Summary

Configures the hardware to send NAK for the next data phase

## Description

This function lets the application send ACK or NAK for the next data from the I2C master

## Precondition

TWIHSx_Initialize must have been called for the associated TWIHS instance.

## Parameters

Param | Description
--- | ---
true | Send NAK to the next data from I2C master
false | Send ACK to the next data from I2C master

## Returns

None

## Example

    TWIHS1_NACKDataPhase(true);

## Remarks

None