Jump to main content

##

# 2.4.18 ADCHS_DMAResultBaseAddrSet Function

## C

    void ADCHS_DMAResultBaseAddrSet(uint32_t baseAddr)

## Summary

Registers the user-defined RAM address at which the DMA engine will start saving the converted data

## Description

Registers the user-defined RAM address at which the DMA engine will start saving the converted data

## Precondition

ADCHS_Initialize() must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
baseAddr | Physical address of the user-defined RAM address

## Returns

None.

## Example

    __COHERENT uint16_t adcResultBuffer[4];
    ADCHS_DMAResultBaseAddrSet((uint32_t)KVA_TO_PA(adcResultBuffer));

## Remarks

None