Jump to main content

##

# 2.92.4 QMSPIx_TapControlSet Function

## C

    // x - Instance of the QMSPI peripheral

    void QMSPIx_TapControlSet(uint16_t tap_vl, uint32_t tap_ctrl);

## Summary

Set control tap adjustment to QMSPI peripheral.

## Description

Set control tap adjustment to QMSPI peripheral. This is used to adjust the auto-H/W trim if needed.

## Precondition

QMSPI must first be initialized using QMSPIx_Initialize().

## Parameters

Param | Description
--- | ---
tap_vl | Tap value to adjust the auto-H/W trim.
tap_ctrl | Select the tap point for signals, these signals control the interface characteristics

## Returns

None.

## Example

    QMSPI0_TapControlSet(100, 0);

## Remarks

None.