Jump to main content

##

# 2.113.10 SMC_DataRead16 Function

## C

    uint16_t SMC_DataRead16(uint32_t dataAddress)

## Summary

Reads 16-bit data from the External Bus Interface (EBI) address.

## Description

Reads 16-bit data from the External Bus Interface (EBI) address.

## Precondition

None.

## Parameters

Param | Description
--- | ---
dataAddress | External Bus Interface (EBI) address

## Returns

Returns 16-bit data from EBI address

## Remarks

None.