Jump to main content

##

# 3.12.19.3 SEFC_FlashPanelGet Function

## C

    SEFC_FLASH_PANEL SEFC_FlashPanelGet(uint32_t address)

## Summary

Identify the flash panel (SEFC0 or SEFC1) for the given address based on the GPNVM bit.

## Description

This function identifies the flash panel by checking the GPNVM bit and returns SEFC_FLASH_PANEL0 or SEFC_FLASH_PANEL1 depending on which flash panel is currently mapped at the given address.

## Precondition

None

## Parameters

Param | Description
--- | ---
address | FLASH panel to identify.

## Returns

SEFC_FLASH_PANEL - SEFC controller flash panel.

## Example

    SEFC_FLASH_PANEL flash_panel = SEFC_FlashPanelGet(0x500000);