Jump to main content

##

# 2.73.41 NVMCTRL_FLASH_START_ADDRESS Macro

## C

The start address of flash varies based on device family. Refer to the generated header file for the actual start address value.

## Summary

Defines the start address of NVMCTRL Flash.

## Description

This constant defines the start address of Flash. It is recommended for the target application to use this constant instead of hardcoded literals.

## Remarks

None.