Jump to main content

##

# 2.80.22 PDECx_COUNTERCompare0Get Function

## C

    uint16_t PDECx_COUNTERCompare0Get ( void ) // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.

## Summary

Reads Compare 0 register value

## Description

This function reads Compare 0 (CC0) register value. This can be period value of the counter if CTRLA.PEREN bit is set.

## Precondition

PDECx_COUNTERInitialize function must have been called first for the given channel.

## Parameters

None.

## Returns

Returns Compare 0 register value.

## Example

    uint16_t value;
    PDEC_COUNTERInitialize();
    PDEC_COUNTERStart();
    value = PDEC_COUNTERCompare0Get();

## Remarks

None.