Jump to main content

##

# 2.127.10 TSENS_ConversionStatusGet Function

## C

    bool TSENS_ConversionStatusGet(void);

## Summary

Returns the status of the temperature measurement

## Description

This function checks whether temperature measurement is complete.

## Precondition

TSENS_Initialize() function must have been called first for the associated instance

## Parameters

None

## Returns

true - temperature measurement is complete and result is available

false - temperature measurement is not complete or not started

## Example

    bool status = false;
    TSENS_Initialize();
    TSENS_Enable();
    TSENS_ConversionStart();
    status = TSENS_ConversionStatusGet();

## Remarks

This function is used to poll the conversion status. This should be called after conversion is started.