Jump to main content

##

# 2.94.3 RAM_IsBusy Function

## C

    bool RAM_IsBusy( void )

## Summary

Returns the current status of RAM.

## Description

This function always returns false as RAM controller is always ready for a new operation.

## Precondition

None.

## Parameters

None

## Returns

false - RAM controller is always ready for a new operation.

## Example

    uint8_t buffer[256];

    RAM_Write( (uint32_t *) buffer, 256, 0x20000000);

    while(RAM_IsBusy());

## Remarks

None