Jump to main content

##

# 2.23.4 CVR_UpdateValue Function

## C

    void CVR_UpdateValue (uint8_t value);

## Summary

Writes to the CVR value selection bits (4-bits).

## Description

Use this function to change the voltage generated by the CVR peripheral.

## Precondition

None.

## Parameters

Value to be written to CVR value selection bits.

## Returns

None.

## Example

    CVR_UpdateValue(0x07);

## Remarks

None.