Jump to main content

##

# 2.26 Digital-to-Analog Converter Controller (DACC)

This Plib implements software abstraction for DACC Peripheral.

## Library Interface

Digital-to-Analog Converter Controller peripheral library provides the following interfaces:

Functions

Name | Description
--- | ---
DACC_Initialize | Initializes DACC module of the device
DACC_IsReady | Returns the status of readiness of DACC module for new conversion request
DACC_ChannelDataWrite | Converts a Digital data to Analog value
DACC_ChannelSelect | Select the channel of DACC module for new conversion request
DACC_DataWrite | Converts a Digital data to Analog value

Data types and constants

Name | Type | Description
--- | --- | ---
DACC_CHANNEL_NUM | Enum | Identifies the Channel index of DACC module

Note: Not all APIs maybe implemented. See the specific device family section for available APIs.