Jump to main content

##

# 2.64.18 MCANx_MessageRAMConfigSet Function

## C

    void MCANx_MessageRAMConfigSet(uint8_t *msgRAMConfigBaseAddress) // x - Instance of the MCAN peripheral

## Summary

Set the Message RAM Configuration.

## Precondition

MCANx_Initialize must have been called for the associated MCAN instance.

## Parameters

Param | Description
--- | ---
msgRAMConfigBaseAddress | Pointer to application allocated buffer base address.Application must allocate buffer from non-cached contiguous memory and buffer size must be MCANx_MESSAGE_RAM_CONFIG_SIZE

## Returns

None

## Example

    uint8_t messageRAMConfig[MCAN0_MESSAGE_RAM_CONFIG_SIZE]__attribute__((aligned (32))) __attribute__((__section__(".region_nocache")));
    MCAN0_MessageRAMConfigSet(&messageRAMConfig);

## Remarks

None.