Jump to main content

##

# 2.39.7 ECIA_GIRQResultGet Function

## C

    uint8_t ECIA_GIRQResultGet(ECIA_INT_SOURCE int_src)

## Summary

Returns the status of the given interrupt source

## Description

Returns the status of the given interrupt source. The status is returned as 1 if both the interrupt source is active and the corresponding interrupt is enabled. The status is returned as 0 otherwise.

## Precondition

None.

## Parameters

Param | Description
--- | ---
int_src | One of the interrupt source from the enum ECIA_INT_SOURCE

## Returns

1 - Interrupt source is active and interrupt is enabled

0 - Interrupt source is not active or interrupt is disabled

## Example

    uint8_t result = ECIA_GIRQResultGet(ECIA_AGG_INT_SRC_GPIO002)

## Remarks

None