Jump to main content

##

# 2.8.76 CANx_SleepModeEnter Function

## C

    void CANx_SleepModeEnter(void) // x - Instance of the CAN peripheral

## Summary

Puts the CAN Peripheral in sleep mode (clock stop request).

## Precondition

CANx_Initialize and CANx_MessageRAMConfigSet must have been called for the associated CAN instance.

## Parameters

None.

## Returns

None.

## Example

    CAN0_SleepModeEnter();

## Remarks

None.