Jump to main content

##

# 2.113.4 SMC_CommandWrite16 Function

## C

    void SMC_CommandWrite16(uint32_t dataAddress, uint16_t command)

## Summary

Writes 16-bit command to the External Bus Interface (EBI) address.

## Description

Writes 16-bit command to the External Bus Interface (EBI) address.

## Precondition

None.

## Parameters

Param | Description
--- | ---
dataAddress | External Bus Interface (EBI) address
command | command to be sent

## Returns

None.

## Remarks

None.