Jump to main content

##

# 2.121.73 TCCx_PWMDeadTimeSet Function

## C

    /* x = TCC instance number */
    void TCCx_PWMDeadTimeSet(uint8_t deadtime_high, uint8_t deadtime_low);

## Summary

Sets the dead time of a given TCC module.

## Description

This function updates low-side and high-side dead time. Dead time values are applicable to all the channels of the TCC module.

## Precondition

TCCx_PWMInitialize function must have been called first for the given channel. And TCC module is in disabled (stopped) state.

## Parameters

Param | Description
--- | ---
deadtime_high | dead-time for high side
deadtime_low | dead-time for low side

## Returns

none

## Example

    TCC0_PWMInitialize();
    TCC0_PWMDeadTimeSet(0x100U, 0x100U);

## Remarks

This function can be called only when TCC module is disabled.