Jump to main content

##

# 2.127.2 TSENS_Enable Function

## C

    void TSENS_Enable(void);

## Summary

Enables given instance of TSENS peripheral

## Description

This function enables TSENS peripheral. This needs to be called before starting temperature measurements.

## Precondition

TSENS_Initialize() function must have been called first for the associated instance

## Parameters

None

## Returns

None.

## Example

    TSENS_Initialize();
    TSENS_Enable();

## Remarks

None.