Jump to main content

##

# 2.18.13 CMPx_DACSlopeWrite Function

## C

    // x is the instance number of the CMP peripheral
    inline static void CMPx_DACSlopeWrite(uint16_t slopeRate)
    {
        DAC1SLPDATbits.SLPDAT = slopeRate;
    }

## Summary

Sets the slope rate.

## Description

This inline function writes sets the slope rate.

## Precondition

None.

## Parameters

Param | Description
slopeRate | inclination rate

## Returns

None.

## Example

    CMP1_DACSlopeWrite(0x10);

## Remarks

Available only in slope mode.