Jump to main content

##

# 3.12.19.7 SEFC_IsBusy Function

## C

    bool SEFC_IsBusy(uint32_t address)

## Summary

Returns the current status of SEFCx controller based on the address passed.

## Description

This function determines the flash panel that is mapped at the given address. It then returns the status of the SEFCx controller, where x is the SEFC flash controller instance associated with the flash panel mapped at the given address.

## Precondition

None.

## Parameters

None.

## Returns

true - If SEFCx peripheral is busy doing an operation.

false - If SEFCx peripheral is ready to accept new request..

## Example

    SEFC_SectorErase( 0x500000 );

    while(SEFC_IsBusy(0x500000));