Jump to main content

##

# 2.3.60 ADC_SoftwareControlledConversionEnable Function

## C

    void ADC_SoftwareControlledConversionEnable(ADC_CORE_NUM core, ADC_CHANNEL_NUM channel)

## Summary

Enables software controlled conversion on the specified ADC core's channel

## Description

Enabling software controlled conversion disables all the hardware triggers and GSWTRG and LSWTRG for all ADC SAR Coren specified by ADCORSEL[1:0] and the channelk specified by ADCHSEL[3:0]. It will place channel k’s conversions under the exclusive control of the SAMP and RQCNVRT bits.

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
core | ADC core n
channel | ADC channel k

## Returns

None

## Example

    ADC_SoftwareControlledConversionEnable(ADC_CORE_NUM1, ADC_CH0);

## Remarks

None