Jump to main content

##

# 3.27.9 Dead Man Timer (DMT)

The primary function of the Deadman Timer (DMT) is to reset the processor in the event of a software mal function. The DMT is a free-running instruction fetch timer, which is clocked whenever an instruction fetch occurs until a count match occurs. Instructions are not fetched when the processor is in Sleep mode.

The DMT consists of a 32-bit counter with a time-out count match value as specified by the DMTCNT<3:0> bits in the DEVCFG1 Configuration register.

A Deadman Timer is typically used in mission critical and safety critical applications, where any single failure of the software functionality and sequencing must be detected

## Library Interface

Dead Man Timer peripheral library provides the following interfaces:

Functions

Name | Description
--- | ---
DMT_Enable | Enables the DMT peripheral
DMT_Disable | Disables the DMT peripheral
DMT_ClearWindowStatusGet | Returns Window is Open flag from the DMT Status Register
DMT_CounterGet | Returns the DMT current counter value
DMT_TimeOutCountGet | Returns the DMT time-out count value
DMT_WindowIntervalGet | Returns the DMT window interval value
DMT_Clear | Restarts the DMT counter