Jump to main content

##

# 2.3.36 ADC_CoreInterruptsStatusGet Function

## C

    void ADC_CoreInterruptsStatusGet(ADC_CORE_NUM core)

## Summary

Returns the specified ADC core's interrupt status

## Description

This function returns the interrupt status of the specified ADC core

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
core | ADC core n

## Returns

Mask of ADC core interrupts. Bitwise OR of the following macros: ADC_CORE_INT_CHRDY_0 ADC_CORE_INT_CHRDY_1 ADC_CORE_INT_CHRDY_2 ADC_CORE_INT_CHRDY_3 ADC_CORE_INT_CHRDY_4 ADC_CORE_INT_CHRDY_5 ADC_CORE_INT_CHRDY_6 ADC_CORE_INT_CHRDY_7 ADC_CORE_INT_EOSRDY ADC_CORE_INT_CHNERRC ADC_CORE_INT_FLTRDY ADC_CORE_INT_CHRDYC ADC_CORE_INT_SOVFL ADC_CORE_INT_CMPHIT

## Example

    ADC_CORE_INT adcCoreIntStatus;
    adcCoreIntStatus = ADC_CoreInterruptsStatusGet(ADC_CORE_NUM1);

## Remarks

None