Jump to main content

##

# 2.46.4 FCW_SingleWordWrite Function

## C

    bool FCW_SingleWordWrite( uint32_t *data, uint32_t address );

## Summary

Writes Two Words into the Flash.

## Description

Writes One Word (4 bytes) at the given address.

## Precondition

None

## Parameters

Param | Description
--- | ---
data | Pointer to the buffer which holds data to be written.
address | Address at which the data will be written.

## Returns

Always return true.

## Example

    uint32_t data[1];

    data[0] = 0x12345678;

    FCW_SingleWordWrite((uint32_t *)data, 0xC088608U);

## Remarks

This Feature may not be available on all devices. Refer to device Datasheet for more information.