Jump to main content

##

# 2.47.29 FLEXCOM_USART_STOP Enum

## C

    /* Blocking, non-blocking and ring buffer mode */

    typedef enum
    {
        FLEXCOM_USART_STOP_1_BIT = FLEX_US_MR_NBSTOP_1_BIT,
        FLEXCOM_USART_STOP_1_5_BIT = FLEX_US_MR_NBSTOP_1_5_BIT,
        FLEXCOM_USART_STOP_2_BIT = FLEX_US_MR_NBSTOP_2_BIT,

        /* Force the compiler to reserve 32-bit memory for each enum */
        FLEXCOM_USART_STOP_INVALID = 0xFFFFFFFF

    } FLEXCOM_USART_STOP;

## Summary

Defines the data type for the FLEXCOM USART peripheral stop bits

## Description

This may be used in the FLEXCOMx_USART_SerialSetup API to change the stop bit configuration

## Remarks

None