Jump to main content

##

# 2.80.8 PDECx_QDECStatusGet Function

## C

    PDEC_QDEC_STATUS PDECx_QDECStatusGet (void) // x is instance of the peripheral and it is applicable only for devices having multiple instances of the peripheral.

## Summary

Identifies status of the quadrature interrupts

## Description

This function returns the status of the interrupts that occur in quadrature mode.

## Precondition

PDECx_QDECInitialize must have been called first.

## Parameters

None

## Returns

PDEC_QDEC_STATUS - status of the quadrature interrupts

## Example

    PDEC_QDEC_STATUS status;
    status = PDEC_QDECStatusGet();

## Remarks

This function is applicable only for quadrature mode.