Jump to main content

##

# 2.3.61 ADC_SyncTriggerCounterSet Function

## C

    void ADC_SyncTriggerCounterSet(uint16_t counterVal)

## Summary

Configures the value of CTRLC.CNT register

## Description

The Synchronous Trigger (STRIG) is driven by a counter at the ADC Control Clock (CTL_CLK) frequency and fires when the counter reaches the value defined by CTRLC.CNT[7:0]. Use this API to set the value of CTRLC.CNT register.

## Precondition

ADCx_Initialize() function must have been called first for the associated instance.

## Parameters

Param | Description
--- | ---
counterVal | value of the CTRLC.CNT

## Returns

None

## Example

    ADC_SyncTriggerCounterSet(0x300);

## Remarks

None