Jump to main content

##

# 2.65.23 MCPWM_CH_STATUS Enum

## C

    typedef enum
    {
        MCPWM_NONE = 0,
        MCPWM_PWMH = _PWMCON1_PWMHIF_MASK,
        MCPWM_PWML = _PWMCON1_PWMLIF_MASK,
        MCPWM_TRG = _PWMCON1_TRGIF_MASK,
        MCPWM_CL = _PWMCON1_CLIF_MASK,
        MCPWM_FLT = _PWMCON1_FLTIF_MASK,
        MCPWM_STATUS_MASK = _PWMCON1_PWMHIF_MASK | _PWMCON1_PWMLIF_MASK | _PWMCON1_TRGIF_MASK | _PWMCON1_CLIF_MASK | _PWMCON1_FLTIF_MASK
    }MCPWM_CH_STATUS;

## Summary

Identifies MCPWM channel event status

## Description

This enumeration identifies MCPWM channel event mask. This can be used to get the status of the events.

## Remarks

None.