Jump to main content

##

# 2.109.3 SENTx_Enable Function

## C

    /* x refers to the instance number */

    void SENTx_Enable(void)

## Summary

Enables the SENTx peripheral of the device.

## Description

This function enables the SENTx Peripheral Library (PLIB) of the device, for its desired use.

## Precondition

The SENTx peripheral must have been initialized using the SENTx_Initialize API. This function should be called when the SENTx peripheral is required to start operation.

## Parameters

None.

## Returns

None.

## Example

    SENTx_Initialize();
    SENTx_Enable();
    /* Perform SENT operations here */

## Remarks

None.