Jump to main content

##

# 2.56.25 I2C_CLIENT_ACK_STATUS Enum

## C

    /* I2C client mode */

    typedef enum
    {

        I2C_CLIENT_ACK_STAT_RECEIVED_ACK = 0,
        I2C_CLIENT_ACK_STAT_RECEIVED_NAK,

    } I2C_CLIENT_ACK_STATUS;

## Summary

I2C Client Acknowledgement Status Enums.

## Description

Defines the enum for the I2C client acknowledgement. Enum of this type is returned by the I2Cx_LastByteAckStatusGet() function.

## Remarks

None.