Jump to main content

##

# 2.109.6 SENTx_IsDataReceived Function

## C

    /* x refers to the instance number */

    bool SENTx_IsDataReceived(void)

## Summary

Checks if data has been received for SENT Peripheral when it acts as a receiver.

## Description

The function returns a boolean value indicating whether new data has been successfully received and is available for processing.

## Precondition

The SENTx peripheral must have been initialized using the SENTx_Initialize API. The peripheral should be enabled using the SENTx_Enable() API.

## Parameters

None.

## Returns

true - SENTx receive completed.

false - SENTx receive not completed.

## Example

    struct SENT_DATA_RECEIVE data;
    SENT1_Initialize();
    data = SENT1_Receive();
    while(!SENT1_IsDataReceived());
    {
    }

## Remarks

None.