Jump to main content

##

# 2.25.1 DAC_CTRL_Initialize Function

## C

    void DAC_CTRL_Initialize(void);

## Summary

Initializes DAC_CTRL module of the device.

## Description

This function initializes DAC_CTRL module of the device with the values configured in MCC GUI. Once the peripheral is initialized, APIs can be used to convert the data.

## Precondition

MCC GUI should be configured with the right values.

## Parameters

None.

## Returns

None.

## Example

    DAC_CTRL_Initialize();

## Remarks

None.