Jump to main content

##

# 2.54.10 HSMCI_ResponseRead Function

## C

    void HSMCI_ResponseRead ( HSMCI_READ_RESPONSE_REG respReg, uint32_t* response )

## Summary

Reads the specified response register

## Description

Response of a command can be read using this API.

## Precondition

A command having a response must have been submitted using the HSMCI_CommandSend() function.

## Parameters

Param | Description
--- | ---
respReg | Enumeration of type HSMCI_READ_RESPONSE_REG identifying the response register to read
response | Pointer to the buffer to read the response into

## Returns

None.

## Example

    uint32_t cmd_response;
    HSMCI_ResponseRead(HSMCI_READ_RESP_REG_0, &cmd_response);

## Remarks

None.