Jump to main content

##

# 2.131.36 USARTx_LIN_FrameSlotEnable Function

## C

    /* x = USART instance number */

    /* Blocking and Ring buffer mode */
    void USARTx_LIN_FrameSlotEnable(bool frameSlotEnable)

## Summary

This API allows the application to Enable/Disable Frame Slot Mode. This mode is useful only for Host nodes.

## Description

This API allows the application to Enable/Disable Frame Slot Mode. This mode is useful only for Host nodes.

## Precondition

USARTx_Initialize must have been called for the associated USART instance.

## Parameters

Param | Description
--- | ---
frameSlotEnable | Enable/Disable checksum true - checksum Enabled false - checksum Disabled

## Returns

None

## Example

    /* LIN frame slot timing is disabled*/
    USART0_LIN_FrameSlotEnable(false);

## Remarks

None